Diagnostic | Description
--- | ---
`a3500fctest`(1M) | In-band diagnostic for Sun StorEdge A3500FC LUNs attached via the host data-path.
`a5ksestest`(1M) | In-band diagnostic for Sun StorEdge A5000 Enclosures attached via the host data-path.
`a5ktest`(1M) | In-band diagnostic for Sun StorEdge A5000 disk drives attached via the host data-path.
`brocadetest`(1M) | Out-of-band diagnostic for testing ports on Brocade Silkworm Fibre Channel switch.
`d2disktest`(1M) | SCSI disk diagnostic for Sun StorEdge D2 SCSI disks.
`daksestest`(1M) | In-band diagnostic for Sun Fire V880 Enclosures attached via the host data-path.
`daktest`(1M) | In-band diagnostic for Sun Fire V880 disk drives attached via the host data-path.
`fcdisktest`(1M) | In-band diagnostic for Internal FC disk drives attached via the host data-path.
`fctapetest`(1M) | In-band diagnostic for FC Tape drives attached via the host data-path.
`ifptest`(1M) | Sun StorEdge PCI FC-100 Host Bus Adapter diagnostic for HBAs using the ifp driver
`qlctest`(1M) | Sun StorEdge PCI Dual Fibre Channel Host Bus Adapter diagnostic for HBAs using the qlc driver.
`socaltest`(1M) | Sun StorEdge SBus FC-100 Host Bus Adapter diagnostic for HBAs using the socal driver.
`linktest`(1M) | The linktest is designed to test two end points of a FC link segment and assist the user in FRU isolation of the link segment. This test is typically run when the FCAL topology indicates a link problem. i.e. A red link.
`switchtest`(1M) | Out-of-band diagnostic for testing ports on Sun StorEdge Network FC switch-8 and switch-16.
`switch2test`(1M) | Out-of-band diagnostic for testing ports on Sun StorEdge Network FC 2 Gigabit switch-8 and switch-16.
`t3test`(1M) | In-band diagnostic for Sun StorEdge T3 and T3+ LUNs attached via the host data-path.
`t3ofdg`(1M) | Out-of-band diagnostic for Sun StorEdge T3 and T3+ LUNs attached via the ethernet connection. t3ofdg will test all of the FRUs within the T3 enclosure
`t3volverify`(1M) | Out-of-band diagnostic for Sun StorEdge T3 and T3+ LUNs attached via the ethernet connection. t3volverify will execute the volume verify function on the selected T3.
`se_configcheck`(1M) | Verify the configuration of a Sun Solution System (3900/6900).
`se2_configcheck`(1M) | Verify the configuration of a Sun Solution System (6320).
`vediag`(1M) | Out-of-band diagnostic for Virtualization Engine (VE) attached via the ethernet connection. Initiates and monitors diagnostics on the virtualization engine.
`veluntest`(1M) | In-band diagnostic for Virtualization Engine VE attached storage. Verifies the functionality of the in-band virtualization engine Sun StorEdge 3900/6900 Series LUN(s).
Exercisors
`stresstest`(1M) | In-band exercisor for all I/O devices attached via a host data-path.
`dex`(1M) | In-band exercisor for all disk and tape drives attached via the host data-path.
`lbf`(1M) | In-band exercisor for FC loops(media) utilized by the host Sun StorEdge HBAs soc+ and QLC 2200.